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Thermal Scope

Inferno 335L features a 384×288 @12μm VOx detector with NETD ≤18 mK and 50Hz frame rate, delivering clear imaging in all conditions. Equipped with a 35mm F0.9 lens, it achieves a detection range of up to 1800m. The built-in 905nm Class 1 laser rangefinder and ballistic calculation ensure accurate shooting. Adopting dual batteries, it supports up to 17 hours of continuous use. With IP67 rating and 1000g shock resistance, it performs reliably with high-caliber firearms in harsh outdoor environments.


Key Features
· 384 × 288 @12 μm VOx thermal detector, NETD ≤18 mK, 50Hz frame rate
· 35mm F0.9 lens, max detection range up to 1800m
· 0.39-inch AMOLED display with 1024×768 resolution, multiple scene modes & color palettes
· 905nm Class 1 laser rangefinder (1.2km, ±1m accuracy) + ballistic calculation & calibration
· Dual battery design, continuous working time ≥17h at 25°C, battery non-polar design for normal operation in forward and reverse installation
· 10 zeroing profiles, rich reticle and aim point options
· IP67 protection, operating temperature: -20°C ~ +50°C, shock resistance up to 1000g/0.4ms
· Wi-Fi connection, 64GB storage, video recording, snapshot and electronic compass supported






n Specification
	Thermal Module
	

	Image Sensor
	UFPA (VOx)

	Resolution
	384×288

	Pixel Pitch
	12µm

	Frame Rate
	50Hz

	NETD
	≤18mk

	Spectral Range
	8-14µm

	Optical Parameter
	

	Focal length / Aperture
	35mm; F0.9

	Field of View
	7.5°×5.6°

	Base Magnification
	3.4X

	Focusing Mode
	Focus Knob

	Eye Relief 
	40mm

	Exit Pupil
	 / 6mm

	Diopter
	+5D to -5D

	Detection Range
	1800m (Human; 3pixels)

	Recognition Range
	450m (Human; 12pixels)

	Image Display
	

	Screen
	AMOLED, 0.39 inch

	Resolution
	1024×768

	Screen Brightness Adjustment
	Support

	Brightness Adjustment
	Support

	Contrast Adjustment
	Support

	Image Enhancement
	Support

	Scene Mode
	City;Plain;Forest

	Display Mode
	Circle;Box

	Color Palette
	White Hot/Black Hot/Red Hot/Fusion/Golden Hot etc.

	Digital Zoom
	1× to 4× step by 0.2×

	 Power Supply
	

	Battery type & Number
	1 built-in 21700 Lithium battery & 1 replaceable 18650 Lithium battery

	External Power Supply
	DC 5V (USB Type-C)

	Battery Operating Time
	≥17h （25℃）

	System
	

	Record Video
	Support

	Capture Snapshot
	Support

	Audio Recording
	Support

	Local Album
	Support

	Recoil Activation Recording 
	Support

	Picture in Picture
	Support

	Hot Track
	Support

	Zeroing Adaptation Mode
	Support

	Screen Adaptation
	-

	Standby Mode
	Support

	Ballistic Calculation
	Support

	Ballistic Calibration
	Support

	Distance Measurement
	Support

	Zeroing Profiles
	10

	Reticle Pattern
	8

	Reticle Pattern
	6

	Aim Point Type
	3

	Aim Point Colour
	6

	BC Aim Point Type
	5

	BC Aim Point Colour
	4

	Ranging Cursor Type
	3

	Ranging Cursor Colour
	3

	 Peripheral
	

	Electronic Compass
	Support

	Attitude Sensor
	Support

	WIFI /APP
	Support; 2.4G

	Storage
	Built-in EMMC (64GB)

	Laser Rangefinder
	905nm;Class 1 Laser Safety 

	Ranging Distance & Accuracy
	1.2 Km*; ±1m

	General
	

	Data Transmission Interface 
	USB (Type-C)

	Protection Level 
	IP67

	Operating Temperature
	-20°C to +50°C

	Max. Recoil
	1000g/0.4ms

	Weight（without battery）
	≤935g

	Dimension
	383×90×86（mm）
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