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LYCAN LN635L 
Thermal Scope

Thermal Image Scope is equipped with a 384 x 288 thermal detector and a 1024 × 768 AMOLED display. Boasting ultra-high thermal sensitivity, it delivers clear target recognition even in harsh weather and low temperature difference scenarios. Featuring long battery life and a maximum observation distance of 2600m, this scope is ideal for hunting, outdoor patrol, search and rescue.


Key Features
· 384×288 resolution with 12 μm sensor, 50Hz frame rate
· High sensitivity thermal module NETD ≤ 15 mK (25°C, F# = 0.9)
· 1024 × 768 resolution 0.49-inch AMOLED display
· 35mm F1.0 lens, observation distance up to 2600 m
· Up to 10 hours of continuous operation at 25°C
· 4 replaceable and rechargeable Li-ion batteries, battery non-polar design for normal operation in forward and reverse installation
· Built-in 905nm Class 1 laser rangefinder (1.2km, ±1m accuracy) and ballistic calculation
· Supports audio recording, snapshot and recoil-activated recording
· IP67 protection grade, operating temperature: -20°C ~ +50°C
· High shock resistance up to 1000 g/0.4 ms
· Wi-Fi connection and 64GB built-in storage available





n Specification
	Item category
	LYCAN LN335L

	Thermal Module
	

	Image Sensor
	UFPA (VOx)

	Resolution
	384×288

	Pixel Pitch
	12µm

	Frame Rate
	50Hz

	NETD
	≤18mk

	Spectral Range
	8-14µm

	Optical Parameter
	

	Focal length / Aperture
	35mm; F1.0

	Field of View
	7.5°×5.6°

	Base Magnification
	3.5X

	Focusing Mode
	Focus Knob

	Eye Relief 
	48mm

	Exit Pupil
	6mm

	Diopter
	+5D to -5D

	Detection Range
	1800m (Human; 3pixels)

	Recognition Range
	450m (Human; 12pixels)

	Image Display
	

	Screen
	AMOLED, 0.49 inch

	Resolution
	1920×1080

	Screen Brightness Adjustment
	Support

	Brightness Adjustment
	Support

	Contrast Adjustment
	Support

	Image Enhancement
	Support

	Scene Mode
	City;Plain;Forest

	Display Mode
	Circle;Box

	Color Palette
	White Hot/Black Hot/Red Hot/Fusion/Golden Hot etc.

	Digital Zoom
	1×; 2×; 4×; 8×

	 Power Supply
	

	Battery type & Number
	4 replaceable 18350 Lithium batteries

	External Power Supply
	DC 5V (USB Type-C)

	Power Consumption
	≤1.9W（25℃）

	Battery Operating Time
	≥12h （25℃）

	System
	

	Record Video
	Support

	Capture Snapshot
	Support

	Audio Recording
	Support

	Local Album
	Support

	Recoil Activation Recording 
	Support

	Picture in Picture
	Support

	Hot Track
	Support

	Zeroing Adaptation Mode
	Support

	Screen Adaptation
	-

	Standby Mode
	Support

	Ballistic Calculation
	Support

	Ballistic Calibration
	Support

	Distance Measurement
	Support

	Zeroing Profiles
	10

	Reticle Pattern
	8

	Reticle Pattern
	6

	Aim Point Type
	3

	Aim Point Colour
	6

	BC Aim Point Type
	5

	BC Aim Point Colour
	4

	Ranging Cursor Type
	3

	Ranging Cursor Colour
	3

	 Peripheral
	

	Electronic Compass
	Support

	Attitude Sensor
	Support

	WIFI /APP
	Support; 2.4G

	Storage
	Built-in EMMC (64GB)

	Laser Rangefinder
	905nm;Class 1 Laser Safety 

	Ranging Distance & Accuracy
	1.2 Km*; ±1m

	General
	

	Data Transmission Interface 
	USB (Type-C)

	Protection Level 
	IP67

	Operating Temperature
	-20°C to +50°C

	Max. Recoil
	1000g/0.4ms

	Weight（without battery）
	≤595g

	Dimension
	238×80×65（mm）


[bookmark: _GoBack]

image2.png




image1.jpeg




